# Prepare the seperate z-actuator

## For this section you will need:

### Tools

- 1 precision wire cutters

### Printed Parts

- 1 seperate z-actuator

## Step 1: Removing brim and supports

The seperate z-actuator has some custom supports and a custom brim to remove. These are highlighted in red in the following images.

- Cut the ties inside actuator column (2 total) with the precision wire cutters

Previous page | Next page