- Build the high-resolution microscope
- Build the low-cost microscope
- Build the upright microscope
- Customisations and alternatives
- Troubleshooting
- Knowledge base

# Workaround: removing the Pi camera lens without the official tool

The official Raspberry Pi Camera Module v2.1 now comes supplied with a white, injection-moulded tool allowing the fixed-focus lens to be adjusted or removed. This tool is much better than the printed tool we relied on in previous versions of the microscope. However, some suppliers do not include the lens tool, in which case you will either need to 3D print picamera2_lens_gripper.stl:

Note that this will not fit v1 of the camera module, which has three lugs rather than four. Also, be sure to use the top surface of the part, i.e. the side that sits on the print bed should face away from the camera module. This is because any "elephant's foot" will cause it to be slightly the wrong shape.

If you cannot print the lens gripper, or if for some reason it doesn't work, you can also gently grip the lens with needlenose pliers to unscrew it. However, it is very easy to damage the module accidentally when doing this, so we don't recommend it.