- Build the high-resolution microscope
- Build the low-cost microscope
- Build the upright microscope
- Customisations and alternatives
- Troubleshooting
- Knowledge base

# Prepare the separate z-actuator

## For this section you will need:

### Tools

- 1 precision wire cutters

### Printed Parts

- 1 separate z-actuator

## Step 1: Removing brim and supports

The separate z-actuator has some custom supports and a custom brim to remove. These are highlighted in red in the following images.

- Cut the ties inside actuator column (2 total) with the precision wire cutters

Previous page | Next page