# Test your printer

If you have bought the plastic parts you can skip this step!

## For this section you will need:

### Tools

- 1 RepRap-style printer

### Materials

- 5 g of PLA filament

## Step 1: Set your printer settings

All microscope parts can be printed out of PLA filament on most RepRap-style printers.

We recommend the following printer settings:

Setting | Value
--- | ---
Material | PLA
Layer height | 0.2mm or less
Supports | None
Infill | Printer default
Brim | Recommended for all part except main body.

Do not print with supports. The microscope has been designed to print without supports. Supports will damage the mechanism.

NOTE: The microscope body has a custom brim included in the STL. This may require custom print settings.

## Step 2: Testing your printer

Now we will test whether your printer can print the bridges in the microscope. Download and print the leg test file this will only use about 5 grams of PLA:

The result should look like this (this has been printed with a brim):

Previous page | Next page