- Constructing the Delta Stage with transmission illumination
- Constructing the Delta Stage with reflection illumination

# 10mm Stage riser

This raises the stage up by 10mm, for longer objective lenses on the OpenFlexure Delta Stage

### Parts

- 5 M3x6mm screw

### Tools

- 1 2.5mm hex screwdriver

### 3D printed parts

- 1 10mm riser
- 2 sample clip - Both sample clips are in the one file.

# Method

## Step 1: Attach the petri dish holder to the stage

Screw the 10mm riser to the main body with three M3x6mm screws using a 2.5mm hex screwdriver.

## Step 2: Attach the sample clips

Screw the sample clips to the 10mm riser using two M3x6mm screws using a 2.5mm hex screwdriver.