- Constructing the Delta Stage with transmission illumination
- Constructing the Delta Stage with reflection illumination

The delta stage is a 3D printed x-y-z translation stage. As the optics do not move it is particularly suited to more complex imaging (phase, reflection, fluorescence microscopy). There are two standard ways to build it, with either transmission illumination or reflection illumination. The motorised translation stage, which forms the main body of the microscope, is the same for both, and so swapping between the two configurations is possible by replacing the optics module. There are also some optional components linked at the bottom of the page.

## Publications

We have described the OpenFlexure Delta Stage's design and possible optical configurations in Optics Express. You can find more related publications and media articles on the OpenFlexure website.

## Printing guidance

We normally print with PLA using a 0.15 layer height and ~18% infill. You should not need to print any of the parts with adhesion settings (brim etc.) or supports. Take note of the optics parts we recommend you print with black PLA, to reduce stray light.

## Building the Delta Stage

There are two versions of the instructions:

- Delta stage microscope with transmission illumination
- Delta stage microscope with reflection illumination

### Optional components

- Simple base: Base with nothing inside; matches the footprint of the OpenFlexure Delta stage exactly.
- Infinity corrected transmission optics module casing: If you are using infinity corrected objective lenses, you will need to use this version of the optics module casing.
- Stage adapters: Adapters for the stage to hold different components.
- LED Grid illumination: For more complex illumination.

### Software

You can control your microscope using the OpenFlexure software. The geometry of the Delta Stage is different to the standard OpenFlexure Microscope. So that the movement of the stage is correct, you will need to change the stage configuration:

1. In OpenFlexure Connect, when connected to your Delta Stage microscope, click `Settings`.
2. Under `MICROSCOPE SETTINGS`, click `Stage`.
3. Change the `Stage geometry` dropdown to `SangaStage (Delta)`.
4. Click `CHANGE STAGE GEOMETRY`.

## Design notes

- Stage geometry