- Build the high-resolution microscope
- Build the low-cost microscope
- Build the upright microscope
- Customisations and alternatives
- Troubleshooting
- Knowledge base

# Attach the sample clips

## For this section you will need:

### Parts

- 1 Sample clips

### Tools

- 1 2.5mm Ball-end Allen key

### Mechanical Components

- 2 M3x10 cap head screws

## Step 1: Prepare the sample clips

- Take one sample clip.
- Insert an M3x10 cap screw through the hole at the end of the clip.
- Repeat for the other clip

## Step 2: Attaching the sample clips

- Insert a 2.5mm Ball-end Allen key through the hole in the curved part of a clip, and into the screw.
- Screw the clip down onto the microscope stage.
- Repeat for the other clip.

Previous page | Next page