- Build the high-resolution microscope
- Build the low-cost microscope
- Build the upright microscope
- Customisations and alternatives
- Troubleshooting
- Knowledge base

# LED Holder: additional print

If you don't have the illumination PCB, you will need to print an extra part to hold a 5mm LED instead.

## For this section you will need:

### Tools

- 1 RepRap-style printer

### Materials

- 5 grams of PLA filament

## Step 1: Print the condenser LED holder

Using a RepRap-style printer and some PLA filament, print condenser LED holder.stl.

Previous page | Next page