# Mount the optics and the microscope

## For this section you will need:

### Tools

- 1 2.5mm Allen key - - Must be a ball-ended key

### Sub-Assemblies

- 1 compete optics module
- 1 microscope with assembled actuators
- 1 prepared microscope stand

### Mechancial Components

- 4 M3x8 cap head screws

## Step 1: Mount the optics

- Get the 2.5mm Allen key ready
- Take the compete optics module and pass it through the bottom of the microscope.
- Insert exposed the mounting screw on the optics module through the keyhole on the z-actuator.
- Insert the Allen key through the teardrop shaped hole on the front of the microscope. Until it engages with the mounting screw.
- Slide optics module up the keyhole as high as it will go while still keeping the Allen key engaged with the screw. Note: this is not the top of the keyhole
- Tighten the screw with the Allen key to lock the optics in place

## Step 2: Mount the microscope

- Place the microscope onto the microscope stand.
- The lugs on the microscope should sit on the lugs of the stand.
- Use four M3x8 cap head screws to fix the microscope in place using the same Allen key

Previous page | Next page